<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="27.94" y1="10.16" x2="86.34" y2="10.16" width="0" layer="20"/>
<wire x1="86.34" y1="10.16" x2="85.07" y2="88.57" width="0" layer="20"/>
<wire x1="85.07" y1="88.57" x2="27.94" y2="88.57" width="0" layer="20"/>
<wire x1="27.94" y1="88.57" x2="27.94" y2="10.16" width="0" layer="20"/>
</plain>
<libraries>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="QS">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="hc05bluetooth">
<description>&lt;b&gt;DIY Modules for Arduino, Raspberry Pi, CubieBoard etc.&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
The library contains a list of symbols and footprints for popular, cheap and easy-to-use electronic modules.&lt;br&gt;
The modules are intend to work with microprocessor-based platforms such as &lt;a href="http://arduino.cc"&gt;Arduino&lt;/a&gt;, &lt;a href="http://raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt;, &lt;a href="http://cubieboard.org/"&gt;CubieBoard&lt;/a&gt;, &lt;a href="http://beagleboard.org/"&gt;BeagleBone&lt;/a&gt; and many others. There are many manufacturers of the modules in the world. Almost all of them can be bought on &lt;a href="ebay.com"&gt;ebay.com&lt;/a&gt;.&lt;br&gt;
&lt;br&gt;
By using this library, you can design a PCB for devices created with usage of modules. Even if you do not need to create PCB design, you can also use the library to quickly document your work by drawing schematics of devices built by you.&lt;br&gt;
&lt;br&gt;
The latest version, examples, photos and much more can be found at: &lt;b&gt;&lt;a href="http://diymodules.org/eagle"&gt;diymodules.org/eagle&lt;/a&gt;&lt;/b&gt;&lt;br&gt;&lt;br&gt;
Comments, suggestions and bug reports please send to: &lt;b&gt;&lt;a href="mailto:eagle@diymodules.org"&gt;eagle@diymodules.org&lt;/b&gt;&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Version: 1.8.0 (2017-Jul-02)&lt;/i&gt;&lt;br&gt;
&lt;i&gt;Created by: Miroslaw Brudnowski&lt;/i&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Released under the Creative Commons Attribution 4.0 International License: &lt;a href="http://creativecommons.org/licenses/by/4.0"&gt;http://creativecommons.org/licenses/by/4.0&lt;/a&gt;&lt;/i&gt;
&lt;br&gt;&lt;br&gt;
&lt;center&gt;
&lt;a href="http://diymodules.org/eagle"&gt;&lt;img src="http://www.diymodules.org/img/diymodules-lbr-image.php?v=1.8.0" alt="DIYmodules.org"&gt;&lt;/a&gt;
&lt;/center&gt;</description>
<packages>
<package name="WIRELESS-BLUETOOTH-HC-05">
<description>&lt;b&gt;Bluetooth Transceiver Module&lt;/b&gt; based on &lt;b&gt;HC-05&lt;/b&gt; board</description>
</package>
</packages>
</library>
<library name="con-headers-jp">
<description>&lt;b&gt;Male(J), Female(P) and Pin Headers&lt;/b&gt;&lt;p&gt;Version 1.02 - 03/10/2009&lt;p&gt;
This library is a collection of various pin headers and AMP, Molex and 3M board-to-board connectors. 
This library assumes the notion of JACKS(male) and PLUGS(female) as represented by the J and P symbols.
Standard male/female pin header types are available in common 0.1" and 2 mm pitch types with alternate mirrored footprints as well.
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="SIP-100-03-32">
<description>&lt;b&gt;SIP Header&lt;/b&gt; - 0.1", 32 mil drill</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="lm35">
<description>Sensores de Temperatura</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ATMEGA328P-PU">
<packages>
<package name="DIP254P762X457-28">
</package>
</packages>
</library>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C7.5B6">
<description>&lt;B&gt;MKS3&lt;/B&gt;, 10 x 6 mm, grid 7.62 mm</description>
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE07">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-ptr500">
<description>&lt;b&gt;PTR Connectors&lt;/b&gt;&lt;p&gt;
Aug. 2004 / PTR Meßtechnik:&lt;br&gt;
Die Bezeichnung der Serie AK505 wurde geändert.&lt;br&gt;
Es handelt sich hierbei um AK500 in horizontaler Ausführung.&lt;p&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;Alte Bezeichnung&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;Neue Bezeichnung&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;AK505/2,grau&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#0000FF"&gt;AK500/2-5.0-H-GRAU&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;AK505/2DS,grau&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#0000FF"&gt;AK500/2DS-5.0-H-GRAU&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;AKZ505/2,grau&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#0000FF"&gt;AKZ500/2-5.08-H-GRAU&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
  &lt;/TABLE&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="AK500/2-H">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
Aug. 2004 / PTR Meßtechnik:&lt;br&gt;
Die Bezeichnung der Serie AK505 wurde geändert.&lt;br&gt;
Es handelt sich hierbei um AK500 in horizontaler Ausführung.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CRISTAL" library="special" package="QS" value=""/>
<element name="HC05" library="hc05bluetooth" package="WIRELESS-BLUETOOTH-HC-05" value="WIRELESS-BLUETOOTH-HC-05"/>
<element name="HUMIDITY" library="con-headers-jp" package="SIP-100-03-32" value="F-1X03-SIP-100-32"/>
<element name="IC1" library="linear" package="TO220V" value="7805TV"/>
<element name="LM35" library="lm35" package="TO92" value="LM35CZ"/>
<element name="PULSE_SPO2" library="con-lsta" package="FE07" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="RESET" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="MPN" value="B3F-1000"/>
</element>
<element name="U1" library="ATMEGA328P-PU" package="DIP254P762X457-28" value="ATMEGA328P-PU">
<attribute name="PRICE" value="None"/>
<attribute name="MF" value="Microchip"/>
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="PACKAGE" value="PDIP-28 Microchip"/>
<attribute name="DESCRIPTION" value=" Embedded microcontroller ATMEGA328P-PU PDIP 28 Microchip Technology 8-Bit 20 MHz I/O number 23 "/>
<attribute name="MP" value="ATMEGA328P-PU"/>
</element>
<element name="CAPIN" library="capacitor-wima" package="C7.5B6" value=""/>
<element name="CAPOUT" library="capacitor-wima" package="C7.5B6" value=""/>
<element name="R1" library="eagle-ltspice" package="0207/10" value="">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R1BL" library="eagle-ltspice" package="0207/10" value="1k">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R2BL" library="eagle-ltspice" package="0207/10" value="2k">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R2" library="eagle-ltspice" package="0207/10" value="">
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="R3" library="eagle-ltspice" package="0207/10" value="">
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="R4" library="eagle-ltspice" package="0207/10" value="">
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="CAPOUT1" library="capacitor-wima" package="C7.5B6" value=""/>
<element name="CAPOUT2" library="capacitor-wima" package="C7.5B6" value=""/>
<element name="X2" library="con-ptr500" package="AK500/2-H" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
</elements>
<signals>
<signal name="9V">
<contactref element="IC1" pad="1"/>
<contactref element="CAPIN" pad="1"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="2"/>
<contactref element="RESET" pad="1"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="8"/>
<contactref element="CAPIN" pad="2"/>
<contactref element="CAPOUT" pad="2"/>
<contactref element="HUMIDITY" pad="1"/>
<contactref element="RESET" pad="2"/>
<contactref element="HC05" pad="4"/>
<contactref element="R2BL" pad="1"/>
<contactref element="PULSE_SPO2" pad="7"/>
<contactref element="CAPOUT2" pad="1"/>
<contactref element="CAPOUT1" pad="1"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="5V">
<contactref element="IC1" pad="3"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="20"/>
<contactref element="CAPOUT" pad="1"/>
<contactref element="HUMIDITY" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="HC05" pad="5"/>
<contactref element="PULSE_SPO2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="RESET" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="RESET" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="9"/>
<contactref element="CRISTAL" pad="2"/>
<contactref element="CAPOUT1" pad="2"/>
</signal>
<signal name="LM35V0">
<contactref element="LM35" pad="2"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="HUMOUT">
<contactref element="HUMIDITY" pad="2"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="16"/>
<contactref element="HC05" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="HC05" pad="2"/>
<contactref element="R2BL" pad="2"/>
<contactref element="R1BL" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="CRISTAL" pad="1"/>
<contactref element="U1" pad="10"/>
<contactref element="CAPOUT2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R1BL" pad="1"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="28"/>
<contactref element="PULSE_SPO2" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="27"/>
<contactref element="PULSE_SPO2" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="4"/>
<contactref element="PULSE_SPO2" pad="4"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="LMGND">
<contactref element="U1" pad="14"/>
<contactref element="LM35" pad="3"/>
</signal>
<signal name="LM5V">
<contactref element="LM35" pad="1"/>
<contactref element="U1" pad="15"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
