| LCD Library 1.3.0 LCD Library - LCD control class hierarchy library. Drop in replacement for the LiquidCrystal Library.

- Main Page
- Classes
- Files

- File List
- File Members

Functions
FastIO.cpp File Reference
`#include "FastIO.h"`

Go to the source code of this file.

## Functions
int | fio_digitalRead (fio_register pinRegister, uint8_t pinBit)
void | fio_digitalWrite (fio_register pinRegister, fio_bit pinBit, uint8_t value)
fio_bit | fio_pinToBit (uint8_t pin)
fio_register | fio_pinToInputRegister (uint8_t pin)
fio_register | fio_pinToOutputRegister (uint8_t pin, uint8_t initial_state)
void | fio_shiftOut (fio_register dataRegister, fio_bit dataBit, fio_register clockRegister, fio_bit clockBit)
void | fio_shiftOut (fio_register dataRegister, fio_bit dataBit, fio_register clockRegister, fio_bit clockBit, uint8_t value, uint8_t bitOrder)
void | fio_shiftOut1 (uint8_t pin, uint8_t value, boolean noLatch)
void | fio_shiftOut1 (fio_register shift1Register, fio_bit shift1Bit, uint8_t value, boolean noLatch)
void | fio_shiftOut1_init (fio_register shift1Register, fio_bit shift1Bit)
void | fio_shiftOut1_init (uint8_t pin)

## Function Documentation

int fio_digitalRead | ( | fio_register | pinRegister,
|  | fio_bit | pinBit
| ) |  |

direct digital read without any checks falls back to normal digitalRead if fast io is disabled

Parameters:

  pinRegister[in] | Register - ignored if fast io is disabled
  pinBit[in] | Bit - Pin if fast io is disabled

Returns:
  Value read from pin

Definition at line 95 of file FastIO.cpp.

void fio_digitalWrite | ( | fio_register | pinRegister,
|  | fio_bit | pinBit,
|  | uint8_t | value
| ) |  |

direct digital write without any checks falls back to normal digitalWrite if fast io is disabled

Parameters:

  pinRegister[in] | Register - ignored if fast digital write is disabled
  pinBit[in] | Bit - Pin if fast digital write is disabled
  value[in] | desired output

Definition at line 76 of file FastIO.cpp.

fio_bit fio_pinToBit | ( | uint8_t | pin | ) |

Find the bit which belongs to specified pin if fast digitalWrite is disabled this function returns the pin

Parameters:

  pin[in] | Number of a digital pin

Returns:
  Bit

Definition at line 65 of file FastIO.cpp.

fio_register fio_pinToInputRegister | ( | uint8_t | pin | ) |

Get the input register for specified pin. if fast digital IO is disabled this function returns NULL

Parameters:

  pin[in] | Number of a digital pin

Returns:
  Register

Definition at line 52 of file FastIO.cpp.

fio_register fio_pinToOutputRegister | ( | uint8_t | pin,
|  | uint8_t | initial_state = `LOW`
| ) |  |

Get the output register for specified pin. if fast digital IO is disabled this function returns NULL

Parameters:

  pin[in] | Number of a digital pin

Returns:
  Register

Definition at line 35 of file FastIO.cpp.

void fio_shiftOut | ( | fio_register | dataRegister,
|  | fio_bit | dataBit,
|  | fio_register | clockRegister,
|  | fio_bit | clockBit
| ) |  |

faster shift out clear using fast digital write falls back to normal digitalWrite if fastio is disabled

Parameters:

  dataRegister[in] | Register of data pin - ignored if fast digital write is disabled
  dataBit[in] | Bit of data pin - Pin if fast digital write is disabled
  clockRegister[in] | Register of data pin - ignored if fast digital write is disabled
  clockBit[in] | Bit of data pin - Pin if fast digital write is disabled

Definition at line 159 of file FastIO.cpp.

void fio_shiftOut | ( | fio_register | dataRegister,
|  | fio_bit | dataBit,
|  | fio_register | clockRegister,
|  | fio_bit | clockBit,
|  | uint8_t | value,
|  | uint8_t | bitOrder
| ) |  |

faster shift out using fast digital write falls back to normal digitalWrite if fastio is disabled

Parameters:

  dataRegister[in] | Register of data pin - ignored if fast digital write is disabled
  dataBit[in] | Bit of data pin - Pin if fast digital write is disabled
  clockRegister[in] | Register of data pin - ignored if fast digital write is disabled
  clockBit[in] | Bit of data pin - Pin if fast digital write is disabled
  bitOrder[in] | bit order

Definition at line 108 of file FastIO.cpp.

void fio_shiftOut1 | ( | uint8_t | pin,
|  | uint8_t | value,
|  | boolean | noLatch = `false`
| ) |  |

one wire shift out protocol needs initialisation (fio_shiftOut1_init)

Parameters:

  pin[in] | digital pin
  value[in] | value to shift out, last byte is ignored and always shifted out LOW

Definition at line 264 of file FastIO.cpp.

void fio_shiftOut1 | ( | fio_register | shift1Register,
|  | fio_bit | shift1Bit,
|  | uint8_t | value,
|  | boolean | noLatch = `false`
| ) |  |

one wire shift out protocol needs initialisation (fio_shiftOut1_init)

Parameters:

  shift1Register[in] | pins register
  shift1Bit[in] | pins bit
  value[in] | value to shift out, last byte is ignored and always shifted out LOW

Definition at line 190 of file FastIO.cpp.

void fio_shiftOut1_init | ( | fio_register | shift1Register,
|  | fio_bit | shift1Bit
| ) |  |

initializes one wire shift out protocol Puts pin to HIGH state and delays until Capacitors are charged.

Parameters:

  shift1Register[in] | pins register
  shift1Bit[in] | pins bit

Definition at line 181 of file FastIO.cpp.

void fio_shiftOut1_init | ( | uint8_t | pin | ) |

initializes one wire shift out protocol Puts pin to HIGH state and delays until Capacitors are charged.

Parameters:

  pin[in] | digital pin

Definition at line 176 of file FastIO.cpp.

All Classes Files Functions Variables Typedefs Enumerations Enumerator Defines