<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22.86" y2="0" width="0" layer="20"/>
<wire x1="22.86" y1="0" x2="22.86" y2="34.544" width="0" layer="20"/>
<wire x1="22.86" y1="34.544" x2="0" y2="34.544" width="0" layer="20"/>
<wire x1="0" y1="34.544" x2="0" y2="0" width="0" layer="20"/>
<text>D2</text>
<text>Q1</text>
<text>U2</text>
<text>U1</text>
<text>J1=12VRUN/P86/L+
J2=GND/15mmBOLT
J3=ECU_OC_IN/P85   
J4=RLY_OC_OUT/L-
J5=PROGRAM_IN</text>
<text>rev5 20190619</text>
<text>+12V
Eng run
@P86
@COIL+
</text>
<text>ECU_IN
Open coll
insideECU
@P85</text>
<text>GND_IN
Pigtail</text>
<text>@COIL-
</text>
<text>D4</text>
<text>P</text>
<text>V</text>
<text>B</text>
<text>PRE
SSU
RE-
PRI
NCI
PLE</text>
<text>B</text>
<text>V</text>
<text>P</text>
<text>See text</text>
<text>-------</text>
<text>-----</text>
<text>See text</text>
</plain>
<libraries>
<library name="DigiKey-UL-Kemet-T491A334K035AT">
<packages>
<package name="CAPT3216N-L">
</package>
</packages>
</library>
<library name="DigiKey-UL-CC0603KRX7ROBB104">
<packages>
<package name="YAG_CC0603">
</package>
</packages>
</library>
<library name="DigiKey-UL-Diode-Comchip-CDBA140SLHF">
<packages>
<package name="CDBA-HF">
<description>Diode, 1A, 40V, 0.3Vdrop, Schottky, Comchip Technology CDBA140SL-HF, DO214AC</description>
</package>
</packages>
</library>
<library name="SM6T27AY-DIOM5436X245N">
<packages>
<package name="DIOM5436X245N">
</package>
</packages>
</library>
<library name="DigiKey-UL-Diodes-B0530W">
<description>DIODES B0530W-FDITR-ND SOD123 30V 500mA</description>
<packages>
<package name="SOD123">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="4,16O1,6">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="3,17/1,3">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="DigiKey-UL-YellowLED-Broadcom-HSMY-C170">
<description>BROADCOM-HSMY-C170</description>
<packages>
<package name="LED_HSMX-C170">
</package>
</packages>
</library>
<library name="DigiKey-UL-GreenLED-Broadcom-HSMG-C170">
<description>BROADCOM-HSMG-C170-Green0805</description>
<packages>
<package name="LED_HSMX-C170">
</package>
</packages>
</library>
<library name="DigiKey-UL-OrangeLED-Broadcom-HSMD-C170">
<description>BROADCOM-HSMD-C170-Orange0805</description>
<packages>
<package name="LED_HSMX-C170">
</package>
</packages>
</library>
<library name="DigiKey-UL-BCP5416T">
<packages>
<package name="SOT-223">
</package>
</packages>
</library>
<library name="DigiKey-UL-10k05w0805">
<packages>
<package name="RES_V0805">
</package>
</packages>
</library>
<library name="DigiKey-UL-1k05w0805">
<packages>
<package name="RC0805N">
</package>
</packages>
</library>
<library name="DigiKey-UL-51o05w0805">
<packages>
<package name="RC0805N">
</package>
</packages>
</library>
<library name="DigiKey-UL-330o05w0805">
<packages>
<package name="RC0805N">
</package>
</packages>
</library>
<library name="DigiKey-UL-2p2k05w0805">
<packages>
<package name="RES_V0805">
</package>
</packages>
</library>
<library name="DigiKey-UL-L78L33ABUT">
<description>L78L33ABUT 3.3v 100ma regulator SOT-89</description>
<packages>
<package name="SOT-89">
</package>
</packages>
</library>
<library name="PIC16F18855-E_SS">
<description>&lt;8-bit Microcontrollers - MCU 8-Bit MCU 14KB Flash 1KB RAM 256B EE CIP&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOP65P780X200-28N">
<description>&lt;b&gt;(SS)28-Lead(SSOP)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="DigiKey-UL-220o05w0805">
<packages>
<package name="RES_V0805">
</package>
</packages>
</library>
<library name="DigiKey-UL-510o05w0805">
<packages>
<package name="RC0805N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="DigiKey-UL-Kemet-T491A334K035AT" package="CAPT3216N-L" value="T491A334K035ATCAPT3216N-L">
<attribute name="MANUFACTURER_PART_NUMBER" value="T491A334K035AT"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Kemet"/>
</element>
<element name="C2" library="DigiKey-UL-CC0603KRX7ROBB104" package="YAG_CC0603" value="CC0603KRX7R0BB104">
<attribute name="MANUFACTURER_PART_NUMBER" value="CC0603KRX7R0BB104"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Yageo"/>
</element>
<element name="C3" library="DigiKey-UL-CC0603KRX7ROBB104" package="YAG_CC0603" value="CC0603KRX7R0BB104">
<attribute name="MANUFACTURER_PART_NUMBER" value="CC0603KRX7R0BB104"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Yageo"/>
</element>
<element name="D1" library="DigiKey-UL-Diode-Comchip-CDBA140SLHF" package="CDBA-HF" value="CDBA140SL-HF">
<attribute name="MANUFACTURER_PART_NUMBER" value="CDBA140SLHF"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Comchip"/>
</element>
<element name="D2" library="SM6T27AY-DIOM5436X245N" package="DIOM5436X245N" value="SM6T27AY"/>
<element name="D3" library="DigiKey-UL-Diodes-B0530W" package="SOD123" value="B0530W-7-F">
<attribute name="MANUFACTURER_PART_NUMBER" value="B0530W7F"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Diodes Inc"/>
</element>
<element name="D4" library="DigiKey-UL-Diodes-B0530W" package="SOD123" value="B0530W-7-F">
<attribute name="MANUFACTURER_PART_NUMBER" value="B0530W7F"/>
<attribute name="VENDOR" value="Diodes Inc"/>
</element>
<element name="D5" library="DigiKey-UL-Diodes-B0530W" package="SOD123" value="B0530W-7-F">
<attribute name="MANUFACTURER_PART_NUMBER" value="B0530W7F"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Diodes Inc"/>
</element>
<element name="D6" library="DigiKey-UL-Diodes-B0530W" package="SOD123" value="B0530W-7-F">
<attribute name="MANUFACTURER_PART_NUMBER" value="B0530W7F"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Diodes Inc"/>
</element>
<element name="J1" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="wirepad" package="4,16O1,6" value="WIREPAD4,16O1,6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="wirepad" package="3,17/1,3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5-1" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5-2" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5-3" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5-4" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5-5" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="DigiKey-UL-YellowLED-Broadcom-HSMY-C170" package="LED_HSMX-C170" value="HSMY-C170">
<attribute name="MANUFACTURER_PART_NUMBER" value="HSMYC170"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Avago Technologies"/>
</element>
<element name="LED2" library="DigiKey-UL-GreenLED-Broadcom-HSMG-C170" package="LED_HSMX-C170" value="HSMG-C170">
<attribute name="MANUFACTURER_PART_NUMBER" value="HSMGC170"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Avago Technologies"/>
</element>
<element name="LED3" library="DigiKey-UL-OrangeLED-Broadcom-HSMD-C170" package="LED_HSMX-C170" value="HSMD-C170">
<attribute name="MANUFACTURER_PART_NUMBER" value="HSMDC170"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Avago Technologies"/>
</element>
<element name="Q1" library="DigiKey-UL-BCP5416T" package="SOT-223" value="BCP5416TA">
<attribute name="MANUFACTURER_PART_NUMBER" value="BCP5416TA"/>
<attribute name="VENDOR" value="Diodes Inc"/>
</element>
<element name="R1" library="DigiKey-UL-10k05w0805" package="RES_V0805" value="CRCW080510K0JNEAHP">
<attribute name="MANUFACTURER_PART_NUMBER" value="CRCW080510K0JNEAHP"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Vishay"/>
</element>
<element name="R2" library="DigiKey-UL-2p2k05w0805" package="RES_V0805" value="CRCW08052K20JNEAHP">
<attribute name="MANUFACTURER_PART_NUMBER" value="CRCW08052K20JNEAHP"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Vishay"/>
</element>
<element name="R3" library="DigiKey-UL-1k05w0805" package="RC0805N" value="CRCW08051K00JNEAHP">
<attribute name="MANUFACTURER_PART_NUMBER" value="CRCW08051K00JNEAHP"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Vishay"/>
</element>
<element name="R4" library="DigiKey-UL-51o05w0805" package="RC0805N" value="ERJ-P06J510V">
<attribute name="MANUFACTURER_PART_NUMBER" value="ERJP06J510V"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Panasonic"/>
</element>
<element name="R5" library="DigiKey-UL-330o05w0805" package="RC0805N" value="ERJ-P06J331V">
<attribute name="MANUFACTURER_PART_NUMBER" value="ERJP06J331V"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Panasonic"/>
</element>
<element name="R6" library="DigiKey-UL-2p2k05w0805" package="RES_V0805" value="CRCW08052K20JNEAHP">
<attribute name="MANUFACTURER_PART_NUMBER" value="CRCW08052K20JNEAHP"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Vishay"/>
</element>
<element name="R7" library="DigiKey-UL-2p2k05w0805" package="RES_V0805" value="CRCW08052K20JNEAHP">
<attribute name="MANUFACTURER_PART_NUMBER" value="CRCW08052K20JNEAHP"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Vishay"/>
</element>
<element name="R8" library="DigiKey-UL-220o05w0805" package="RES_V0805" value="CRCW0805220RJNEAHP">
<attribute name="MANUFACTURER_PART_NUMBER" value="CRCW0805220RJNEAHP"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Vishay"/>
</element>
<element name="U1" library="DigiKey-UL-L78L33ABUT" package="SOT-89" value="">
<attribute name="MANUFACTURER_PART_NUMBER" value="L78L33ABUTR"/>
<attribute name="VENDOR" value="STMicroelectronics"/>
</element>
<element name="U2" library="PIC16F18855-E_SS" package="SOP65P780X200-28N" value="">
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU 8-Bit MCU 14KB Flash 1KB RAM 256B EE CIP"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="PIC16F18855-E/SS"/>
<attribute name="MOUSER_PART_NUMBER" value="579-PIC16F18855-E/SS"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=579-PIC16F18855-E%2FSS"/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="RS_PRICE-STOCK" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="DigiKey-UL-510o05w0805" package="RC0805N" value="ERJ-P06J511V">
<attribute name="MANUFACTURER_PART_NUMBER" value="ERJP06J511V"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Panasonic"/>
</element>
</elements>
<signals>
<signal name="PWR_P_12">
<contactref element="D2" pad="C"/>
<contactref element="R7" pad="2"/>
<contactref element="D1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="TO_Q1_BASE">
<contactref element="U2" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="RY_OUT_OC">
<contactref element="Q1" pad="2"/>
<contactref element="D3" pad="2"/>
<contactref element="J4" pad="1"/>
<contactref element="LED3" pad="1"/>
</signal>
<signal name="YEL_LED_PLUS">
<contactref element="D6" pad="1"/>
<contactref element="LED1" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="TO_GRN_LED">
<contactref element="U2" pad="3"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="TO_YEL_LED_HI_R">
<contactref element="R4" pad="1"/>
<contactref element="D6" pad="2"/>
</signal>
<signal name="TO_RESET">
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="J5-1" pad="1"/>
</signal>
<signal name="CMD_IN_RAW_OC">
<contactref element="D4" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="TO_PGM_D">
<contactref element="U2" pad="28"/>
<contactref element="J5-4" pad="1"/>
</signal>
<signal name="TO_PGM_C">
<contactref element="U2" pad="27"/>
<contactref element="J5-5" pad="1"/>
</signal>
<signal name="ORG_LED_PLUS">
<contactref element="R6" pad="1"/>
<contactref element="LED3" pad="2"/>
</signal>
<signal name="PWR_P_3P3">
<contactref element="R1" pad="2"/>
<contactref element="U2" pad="20"/>
<contactref element="J5-2" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="TO_YEL_LED_HI">
<contactref element="U2" pad="4"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="GRN_LED_PLUS">
<contactref element="R5" pad="2"/>
<contactref element="LED2" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="PWR_GND">
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="19"/>
<contactref element="U2" pad="8"/>
<contactref element="Q1" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="LED1" pad="1"/>
<contactref element="LED2" pad="1"/>
<contactref element="J5-3" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="J2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="CMD_IN_PROC">
<contactref element="U2" pad="7"/>
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="D5" pad="1"/>
</signal>
<signal name="PWR_12_RAW">
<contactref element="D1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="D3" pad="1"/>
</signal>
<signal name="BW_ECU_PROT_D">
<contactref element="R9" pad="2"/>
<contactref element="D5" pad="2"/>
<contactref element="D4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
