<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<packages>
<package name="CAPC1608X90">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="C0603C104M5RACTU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="C0603C104M5RACTU" prefix="C">
<description>CAP, X7R, 0.1UF, 50V, 0603</description>
<gates>
<gate name="G$1" symbol="C0603C104M5RACTU"/>
</gates>
<devices>
<device name="" package="CAPC1608X90">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value=" 0.1µF ±20% 50V Ceramic Capacitor X7R 0603 _1608 Metric_ "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="399-7845-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/kemet/C0603C104M5RACTU/399-7845-1-ND/3471568?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="KEMET"/>
<attribute name="MP" value="C0603C104M5RACTU"/>
<attribute name="PACKAGE" value="0603 Kemet"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
