<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<packages>
<package name="RESC1508X50N">
</package>
</packages>
<symbols>
<symbol name="RNCP0603FTD33R2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RNCP0603FTD33R2" prefix="R">
<gates>
<gate name="G$1" symbol="RNCP0603FTD33R2"/>
</gates>
<devices>
<device name="" package="RESC1508X50N">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value=" Res Thin Film 0603 33.2 Ohm 1% 0.125W_1/8W_ ±100ppm/C Sulfur Resistant Pad SMD T/R "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="RNCP0603FTD33R2CT-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/stackpole-electronics-inc/RNCP0603FTD33R2/RNCP0603FTD33R2CT-ND/2240417?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Stackpole Electronics Inc"/>
<attribute name="MP" value="RNCP0603FTD33R2"/>
<attribute name="PACKAGE" value="1508 Stackpole"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
